EZ Street asphalt is a permanent pothole repair that’s easy to install and does not require any special equipment.
Available in 22 kg Bags and One Tonne Bulk Sacks
Sweep out the area to be patched. Make sure to remove all loose debris, dust, unstable base material and broken pieces of pavement (including "alligator" cracked areas).
Fill the pothole with EZ Street asphalt. For potholes deeper than 4", compact material in 2" layers.
Compact with a plate compactor, steel wheel roller, vehicle tire, hand tamp or shovel. The final EZ Street lift should be placed just over the level of the existing pavement allowing for optimal secondary compaction as a result of traffic flow.